{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Issues"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Issues","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"flags":["formulas_cached_only"]}
[]
["Product name","HSB MRTS Kathode-MCP"]
["Board name","MLA-0387-P0"]
[]
["Issue #","Description","Rev","Status [Open/Closed ]","Remarks","Engineer"]
[1,"ADC-IN2 moves to Ext1-4","PA0","Closed",null,"Tla"]
[2,"Extra UART on EXT1-22 and EXT1-23","PA0","Closed",null,"Tla"]
[3,"Replace D8, D9 by GSOT05C","PA0","Closed",null,"Tla"]
[4,"Replace D4-7 by GSOT03C","PA0","Closed",null,"Tla"]
[5,"Replace X4 by Molex 22-23-2081","PA0","Closed",null,"Tla"]
[6,"Tie pin 14 of U4 to Vcc","PA0","Closed",null,"Tla"]
[7,"Replace R9 and R11 by 1k 0,1%. Do the same for the other 2 channels","PA0","Closed",null,"Tla"]
[8,"Place a 1.2nF parallel to R9. Do the same for the other 2 channels","PA0","Closed",null,"Tla"]
[9,"Place a TCJB336M010R0070 parallel to C12, C17, C21","PA0","Closed",null,"Tla"]
[10,"Place a 10nF parallel to R12, R18, R24","PA0","Closed",null,"Tla"]
[11,"Place 1nF parallel to C66, C65, D13,C30, C31, C34, C33, C41, C42, C48, C55, D4-D7","PA0","Closed",null,"Tla"]
[12,"Place a SMJA12A directly over X3","PA0","Closed",null,"Tla"]
[13,"Remove U8","PA0","Closed",null,"Tla"]
[14,"Add a buzzer","PA0","Closed",null,"Tla"]
[15,"Safety features must be implemented in HW","PA0","Closed",null,"Tla"]
[16,"Add labels in silk to all connectors","PA0","Closed","See doc in folder 0387-P0-0-0","Tla"]
[17,"Add a LED","PA0","Closed",null,"Tla"]