{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["BOM","PCB Constraints"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BOM","index":0,"n_rows":65,"n_cols":11,"rows_kept":65,"flags":["formulas_cached_only"]}
[]
[{"$nulls":4},"Bill of Material",null,"Project Title"]
[{"$nulls":6},"PA0"]
[]
[{"$nulls":4},"Project:",null,"MLA-0387-P1.PrjPCB"]
[{"$nulls":4},"Variant:",null,"MLA-0387-A2"]
[null,"H:\\Altium templates","Without further notice all components are RoHS compliant",null,"Work Instruction",null,"H:\\Altium templates"]
[{"$nulls":4},"Report Date:",null,"2-6-2017","09:55:15"]
[{"$nulls":4},"Print Date:",null,"2017-06-02",42888.413516898145]
[null,null,"Designator","Description","Manufacturer","Product nr.","Footprint","Layer","THT","Quantity","Remark"]
[null,null,"C1, C3, C5, C7, C9, C10, C11, C13, C15, C16, C18, C19, C20, C22, C23, C25, C26, C28, C30, C32, C35, C36, C37, C38, C41, C42, C44, C48, C49, C50, C52, C55, C56, C57, C58, C59, C60, C61","Capacitor 100nF 50V X7R 0603","","","C0603","Top","",38,""]
[null,null,"C2, C4, C6","Capacitor 10nF 50V X7R 0603","","","C0603","Top","",3,""]
[null,null,"C8, C12, C17, C21, C24, C27, C29, C31, C33, C34, C40, C43, C45, C46, C47, C51, C53, C54","Capacitor 10uF 25V X7R 1206","","","C1206","Top","",18,""]
[null,null,"C14","Capacitor 100pF 50V C0G 0603","","","C0603","Top","",1,""]
[null,null,"C39","Elco 100uF 20% 25V SMD","Kemet","EXV107M025A9HAA","Kemet_9H","Top","",1,""]
[null,null,"D1, D2","Schottky diode 30V 1A","ON Semiconductor","SS13FL","SOD123F","Top","",2,""]
[null,null,"D3, D4, D5, D6, D7","TVS diode 3V3 dual SOT23","NXP","PESD3V3S2UT,215","SOT-23_3","Top","",5,""]
[null,null,"D8, D9","TVS diode 5V dual SOT23","NXP","PESD3V3S2UAT,215","SOT-23_3","Top","",2,""]
[null,null,"D10, D11, D12","TVS diode 2.8V SOT-23","","SLVU2.8","SOT-23_3","Top","",3,""]
[null,null,"D13","TVS diode 5V dual SOT23","NXP","PESD5V0S2UAT,215","SOT-23_3","Top","",1,""]
[null,null,"F1","OMNI-BLOK 154 Fuse + holder 1.25A","Littelfuse","01541.25DR","OMNI-BLOK 154","Top","",1,""]
[null,null,"FID1, FID2, FID3","FIDUCIAL 2MM","","","FID","Top","",3,""]
[null,null,"L1, L2, L3, L7","Ferrite bead 600 Ohm 500mA 0603","Murata","BLM18AG601","L0603","Top","",4,""]
[null,null,"L5","Inductor 10uH shielded 2.5A","Bourns","SRN6045-100M","SRN6045","Top","",1,""]
[null,null,"L6","Inductor 22uH shielded 1.5A","Bourns","SRN6045-220M","SRN6045","Top","",1,""]
[null,null,"M1, M2, M3","TO-220 heatsink 37.5 mm height","Assmann","V6560X","6560X","Bottom","",3,""]
[null,null,"M7, M8, M9","Isolated, proportional DC to 10kV DC converter 0.5W","XP Power","","Q101-5","Bottom","",3,""]
[null,null,"MH1, MH2, MH3, MH4, MH5, MH6","Mounting hole 3.5mm","","","3.5MM","Top","",6,""]
[null,null,"MH7, MH8, MH9, MH10","Mounting hole 2.5mm","","","2.5MM","Top","",4,""]
[null,null,"PCB1","Bare PCB","MK","MLA-0387-P1-PA0","MK logo","Top","",1,""]
[null,null,"Q1, Q2, Q3","NPN transistor 60V 3A TO-220","ST","2ST31A","TO-220_NPN","Bottom","Yes",3,""]
[null,null,"Q4","N-Channel Enhancement Mode FET 60V 1.2A SOT23","Diodes","DMN6140L","SOT-23_3","Top","",1,""]
[null,null,"R1, R3, R5","Resistor 11k8 0.1% 0603","","","R0603","Top","",3,""]
[null,null,"R2, R4, R6","Resistor 215k 0.1% 0603","","","R0603","Top","",3,""]
[null,null,"R7, R13, R19","Resistor 11k3 0.1% 0603","","","R0603","Top","",3,""]
[null,null,"R8, R14, R20","Resistor 22k6 0.1% 0603","","","R0603","Top","",3,""]
[null,null,"R9, R11, R15, R17, R21, R23","Resistor 49k9 0.1% 0603","","","R0603","Top","",6,""]
[null,null,"R10, R16, R22","Resistor High Voltage 1G 5W 1% axial","Ohmite","MOX-2-121007FE","MOX-2-12","Top","",3,""]
[null,null,"R12, R18, R24","Resistor 249k 0.1% 0603","","","R0603","Top","",3,""]
[null,null,"R25, R28","Resistor 0R 1% 1206","","","1206","Top","",2,""]
[null,null,"R26","Resistor 147k 1% 0603","","","R0603","Top","",1,""]
[null,null,"R27","Resistor 15k8 1% 0603","","","R0603","Top","",1,""]
[null,null,"R29","Resistor 0R075 1% 1206","","","1206","Top","",1,""]
[null,null,"R30, R32","Resistor 9k76 1% 0603","","","R0603","Top","",2,""]
[null,null,"R31","Resistor 113k 1% 0603","","","R0603","Top","",1,""]
[null,null,"R33","Resistor 0R22 1% 1206","","","1206","Top","",1,""]
[null,null,"R34, R41, R42, R43, R44, R45, R46, R51, R52, R61, R62, R65","Resistor 10k 1% 0603","","","R0603","Top","",12,""]
[null,null,"R37, R40, R53, R54, R55, R56, R57, R58, R59, R60, R63, R64","Resistor 330R 1% 0603","","","R0603","Top","",12,""]
[null,null,"R47","Resistor 13k7 1% 0603","","","R0603","Top","",1,""]
[null,null,"R48","Resistor 1k5 1% 0603","","","R0603","Top","",1,""]
[null,null,"R49, R50","Resistor 5R6 5% 1206 1/4W","","","1206","Top","",2,""]
[null,null,"U1, U2","Precision, CMOS Input, RRIO, Wide Supply Range Amplifiers, 14-pin Narrow SOIC, Pb-Free","Texas Instruments","LMP7704MAX/NOPB","D0014A_M","Top","",2,""]
[null,null,"U3","Precision, CMOS Input, RRIO, Wide Supply Range Amplifiers, 8-pin Narrow SOIC, Pb-Free","Texas Instruments","LMP7702MAX/NOPB","D0008A_M","Top","",1,""]
[null,null,"U4","Quad-Ch 12Bit DAC with internal reference and SPI interface","Maxim","","TSSOP-14","Top","",1,""]
[null,null,"U7","Series Voltage Reference IC 2,5V 0,2% 25mA SOT-23-3","Texas Instruments","","SOT-23_3","Top","",1,""]
[null,null,"U8","EEPROM 8kb SPI SO8","ST","","SOP 8L 150MIL","Top","",1,""]
[null,null,"U9, U10","42V, 2A Constant On-Time Switching Regulator with Adjustable Current Limit, 10-pin eMSOP, Pb-Free","Texas Instruments","LM25011MYX/NOPB","10-MSOP-EP","Top","",2,""]
[null,null,"U11","Header 6 pins THT 2.54 mm pitch","","","HDR-6","Bottom","Yes",1,""]
[null,null,"U12","Single Power Supply Quadruple Buffer GATE w/ 3-State Output CMOS Logic Level Shifter","Texas Instruments","SN74LV4T125","PW0014A_M","Top","",1,""]
[null,null,"X1, X2","Receptacle 2x20 pins THT 2.54mm pitch","3M","929975-01-20-RK","929975-01-20-RK","Bottom","Yes",2,""]
[null,null,"X3","Micro-Fit 3.0 header 2 pins RA THT","Molex","43650-0200","43650-0200","Bottom","",1,""]
[null,null,"X4","Receptacle 8 pins THT 2.54mm pitch","Molex","22-18-2081","22-18-2081","Bottom","Yes",1,""]
[null,null,"X5","Header 16 pins THT 2.54mm pitch","","","HDR-16","Top","Yes",1,""]
[null,null,"X6","C-GRID III Boxed Header 2p, 2.54mm pitch","Molex","90136-1102","90136-1102","Bottom","Yes",1,""]
[null,null,"X7","C-GRID III Boxed Header 3p, 2.54mm pitch","Molex","90136-1103","90136-1103","Bottom","Yes",1,""]

{"sheet":"PCB Constraints","index":1,"n_rows":25,"n_cols":7,"rows_kept":25,"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"PCB production constraints",null,"Project Title"]
[{"$nulls":5},"MLA-0387-A2","PA0"]
[]
[{"$nulls":3},"Project:",null,"MLA-0387-P1.PrjPCB"]
[{"$nulls":3},"Variant:",null,"MLA-0387-A2"]
[null,"Without further notice all components are RoHS compliant"]
[{"$nulls":3},"Report Date:",null,"2-6-2017","09:55:15"]
[{"$nulls":3},"Print Date:",null,"2017-06-02",42888.413516898145]
[null,"Constraint type","Constraint"]
[null,"Dimension","300 x 107.5 mm"]
[null,"Number of layers","2"]
[null,"Minimum clearance","0.15 mm"]
[null,"Minimum track width","0.15 mm"]
[null,"Min finished hole size","0.25 mm"]
[null,"Min annular ring","0.175 mm"]
[null,"Finish","Selective Gold"]
[null,"UR logo","No"]
[null,"Color Soldermask","Green"]
[null,"Silkscreen bottom","Yes"]
[null,"Silkscreen color","White"]
[null,"Specific Layer Stackup","No"]
[null,"Edge connectors and surface","No"]
[null,"Board cutouts and minimum drill size","No"]
[null,"Print thickness","1.6 mm"]