{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["Issues"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Issues","index":0,"n_rows":22,"n_cols":6,"rows_kept":22,"flags":["formulas_cached_only"]}
[]
["Product name","[prod name]"]
["Board name","[board name]"]
[]
["Issue #","Description","Rev","Status [Open/Closed ]","Remarks","Engineer"]
[1,"ADC-IN2 moves to Ext1-4","PA0","Open",null,"Tla"]
[2,"Extra UART on EXT1-22 and EXT1-23","PA0","Open",null,"Tla"]
[3,"Replace D8, D9 by GSOT05C","PA0","Open",null,"Tla"]
[4,"Replace D4-7 by GSOT03C","PA0","Open",null,"Tla"]
[5,"Replace X4 by Molex 22-23-2081","PA0","Open",null,"Tla"]
[6,"Tie pin 12 and 14 of U4 to Vcc","PA0","Open",null,"Tla"]
[7,"Replace R9 and R11 by 1k 0,1%. Do the same for the other 2 channels","PA0","Open",null,"Tla"]
[8,"Place a 1.2nF parallel to R9. Do the same for the other 2 channels","PA0","Open",null,"Tla"]
[9,"Place a TCJB336M010R0070 parallel to C12, C17, C21","PA0","Open",null,"Tla"]
[10,"Place 2,7nF parallel to R18 for Tesla variant","PA0","Open",null,"Tla"]
[11,"Place 5,6nF parallel to R12, R18, R24 for Anode variant","PA0","Open",null,"Tla"]
[12,"ReplaceTesla Interlock circuit with Interlock solenoid circuit for driving a relay.","PA0","Open",null,"Tla"]
[13,"Place a 1nF parallel to D13, C61, C60, C29, C31, C34, C33, R12, R18, R24, C41, C42, C48, C55, D4-D7","PA0","Open",null,"Tla"]
[14,"Place a SMJA12A directly over X3","PA0","Open",null,"Tla"]
[15,"Remove U8","PA0","Open",null,"Tla"]
[16,"Add a buzzer","PA0","Open",null,"Tla"]
[17,"Add -3V3 supply and connect opamps V- pins to it. See MLA-0387-P0","PA0","Open","Improves low input voltage performance","Tla"]