{"text_format":"3","workbook":"xls","n_sheets":2,"sheets":["BOM","PCB Constraints"],"not_rendered":{"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BOM","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"flags":["formulas_cached_only"]}
[]
[{"$nulls":4},"Bill of Material",null,"HSB MRTS"]
[{"$nulls":6},"PB1"]
[]
[{"$nulls":4},"Project:",null,"MLA-0387-P1.PrjPCB"]
[{"$nulls":4},"Variant:",null,"MLA-0387-A1"]
[null,"H:\\Altium templates","Without further notice all components are RoHS compliant",null,"Work Instruction",null,"H:\\Altium templates"]
[{"$nulls":4},"Report Date:",null,"5-12-2017","16:32:54"]
[{"$nulls":4},"Print Date:",null,"2017-12-05",43074.689753819446]
[null,null,"Designator","Description","Manufacturer","Product nr.","Footprint","Layer","THT","Quantity","Remark"]
[null,null,"C3","Capacitor 100nF 50V X7R 0603 5%","","","C0603","Top","",1,""]
[null,null,"C4","Capacitor 10nF 50V X7R 0603 5%","","","C0603","Top","",1,""]
[null,null,"C7, C15, C16, C18, C23, C25, C26, C28, C30, C32, C36, C37, C38, C41, C42, C44, C48, C49, C50, C52, C55, C56, C57, C58, C59, C60, C61, C63, C64, C65, C66, C67, C69, C70, C92, C97, C99","Capacitor 100nF 50V X7R 0603","","","C0603","Top","",37,""]
[null,null,"C8, C17, C24, C27, C29, C31, C33, C34, C40, C43, C45, C46, C47, C51, C53, C54, C62","Capacitor 10uF 25V X7R 1206","","","C1206","Top","",17,""]
[null,null,"C14","Capacitor 100pF 50V C0G 0603","","","C0603","Top","",1,""]
[null,null,"C39","Elco 100uF 20% 25V SMD","Kemet","EXV107M025A9HAA","Kemet_9H","Top","",1,""]
[null,null,"C75","CAP TANT POLY 33UF 10V 1210","AVX","TCJB336M010R0070","C1210","Top","",1,""]
[null,null,"C76, C81, C82, C83, C84, C85, C86, C87, C88, C93, C94, C95, C96, C98, C100, C101, C102, C103, C104, C105, C106, C107, C108","Capacitor 1.2nF 50V X7R 0603","","","C0603","Top","",23,""]
[null,null,"C77","Capacitor 2.7nF 50V X7R 0603","","","C0603","Top","",1,""]
[null,null,"C89, C90, C91","Capacitor 4.7uF 16V X7R 1206","Taiyo Yuden","EMK316B7475KL-T","C1206","Top","",3,""]
[null,null,"C109","Capacitor 10nF 50V X7R 0603","","","C0603","Top","",1,""]
[null,null,"D1, D2, D11","Schottky diode 30V 1A","ON Semiconductor","SS13FL","SOD123F","Top","",3,""]
[null,null,"D3, D4, D5, D6, D7, D13, D17","TVS diode 3V3 dual SOT23","Vishay","GSOT03C-E3-08","SOT-23_3","Top","",7,""]
[null,null,"D8, D9","TVS diode 5V dual SOT23","Vishay","GSOT05C-E3-08","SOT-23_3","Top","",2,""]
[null,null,"D14","LED Green/Red Clear 1210","Kingbright","APBD3224ESGC-F01","APBD3224","Top","",1,""]
[null,null,"D15, D18","TVS diode 15V SOT-23","Vishay","GSOT15-E3-08","SOT-23_3","Top","",2,""]
[null,null,"D16","TVS diode 12V 400W Unidir DO-214AC","","SMAJ12A","SMA_DO-214AC","Top","",1,""]
[null,null,"F1","OMNI-BLOK 154 Fuse + holder 1.25A","Littelfuse","01541.25DR","OMNI-BLOK 154","Top","",1,""]
[null,null,"FID1, FID2, FID3, FID4, FID5, FID6","FIDUCIAL 2MM","","","FID","Top","",6,""]
[null,null,"L1, L2, L3, L7, L8","Ferrite bead 600 Ohm 500mA 0603","Murata","BLM18AG601","L0603","Top","",5,""]
[null,null,"L4","WE-SL5 SMD Common Mode Line Filter, 470 uH","Wurth Elektronik","744272471","WE-SL5_sectioinal","Top","",1,""]
[null,null,"L5, L6","Inductor 15uH shielded 1.9A","Bourns","SRN6045-150M","SRN6045","Top","",2,""]
[null,null,"LS1","Audio transducer magnetic 5Vdc","PUI audio","AI-1223-TWT-5V-5-R","Buzzer_12mm","Top","Yes",1,""]
[null,null,"M2","TO-220 heatsink 37.5 mm height","Assmann","V6560X","6560X","Bottom","",1,""]
[null,null,"M4","6kV wire jumper","","","6KV jumper","Top","",1,"Supplied by Photonis"]
[null,null,"M5","STM32F107 development board","Olimex","STM32-H107","","None","",1,""]
[null,null,"MP1, MP2, MP3, MP4, MP5, MP6","WA-SMSI SMT Steel Spacer, M3 Thread Internal, Length 14mm","Wurth Elektronik","9774140360R","9774140360","Top","",6,""]
[null,null,"MP7, MP8, MP9, MP10","WA-SMSI SMT Steel Spacer, M2 Thread Internal, Length 3mm","Wurth Elektronik","9774030243R","9774030243","Top","",4,""]
[null,null,"MP11, MP12, MP13, MP14","WA-SMSI SMT Steel Spacer, M2.5 Thread Internal, Length 8mm","Wurth Elektronik","9774080151R","9774080151","Top","",4,""]
[null,null,"PCB1","Bare PCB","MK","MLA-0387-P1-PB1","MK logo","Top","",1,""]
[null,null,"Q2","NPN transistor 60V 3A TO-220","ST","2ST31A","TO-220_NPN","Bottom","Yes",1,""]
[null,null,"Q4, Q5, Q6","N-Channel Enhancement Mode FET 60V 1.2A SOT23","Diodes","DMN6140L","SOT-23_3","Top","",3,""]
[null,null,"R3","Resistor 11k8 0.1% 0603","","","R0603","Top","",1,""]
[null,null,"R4","Resistor 215k 0.1% 0603","","","R0603","Top","",1,""]
[null,null,"R13","Resistor 11k3 0.1% 0603","","","R0603","Top","",1,""]
[null,null,"R14","Resistor 22k6 0.1% 0603","","","R0603","Top","",1,""]
[null,null,"R15, R17, R90","Resistor 1k 0.1% 0603","","","R0603","Top","",3,""]
[null,null,"R16","Resistor High Voltage 1G 5W 1% axial","Ohmite","MOX-2-121007FE","MOX-2-12","Top","",1,""]
[null,null,"R18","Resistor 412k 0.1% 0603","","","R0603","Top","",1,""]
[null,null,"R26","Resistor 147k 1% 0603","","","R0603","Top","",1,""]
[null,null,"R27","Resistor 15k8 1% 0603","","","R0603","Top","",1,""]
[null,null,"R28, R37, R40, R53, R54, R55, R56, R57, R58, R59, R60, R63, R64, R69, R70, R71, R77, R85, R86","Resistor 330R 1% 0603","","","R0603","Top","",19,""]
[null,null,"R29","Resistor 0R1 1% 1206","","","1206","Top","",1,""]
[null,null,"R30, R32","Resistor 9k76 1% 0603","","","R0603","Top","",2,""]
[null,null,"R31","Resistor 113k 1% 0603","","","R0603","Top","",1,""]
[null,null,"R33","Resistor 0R15 1% 1206","","","1206","Top","",1,""]
[null,null,"R34, R35, R36, R38, R39, R41, R42, R43, R44, R45, R46, R51, R52, R61, R62, R65, R76, R78, R79, R80, R82, R83, R94","Resistor 10k 1% 0603","","","R0603","Top","",23,""]
[null,null,"R50, R66","Resistor 0R 1% 1206","","","1206","Top","",2,""]
[null,null,"R72, R73, R74","Resistor 33R 1% 0603","","","R0603","Top","",3,""]
[null,null,"R88","Resistor 200k 0.1% 0603","","","R0603","Top","",1,""]
[null,null,"R89","Resistor 1.5M 0.1% 0603","","","R0603","Top","",1,""]
[null,null,"U2","Precision, CMOS Input, RRIO, Wide Supply Range Amplifiers, 14-pin Narrow SOIC, Pb-Free","Texas Instruments","LMP7704MAX/NOPB","D0014A_M","Top","",1,""]
[null,null,"U3","Precision, CMOS Input, RRIO, Wide Supply Range Amplifiers, 8-pin Narrow SOIC, Pb-Free","Texas Instruments","LMP7702MAX/NOPB","D0008A_M","Top","",1,""]
[null,null,"U4","Quad-Ch 12Bit DAC with internal reference and SPI interface","Maxim","MAX5715BAUD+","TSSOP-14","Top","",1,""]
[null,null,"U5","Isolated, proportional DC to 6kV DC converter 1W","XP Power","A60P-5","A60P-5","Top","",1,""]
[null,null,"U7","Series Voltage Reference IC 2,5V 0,2% 25mA SOT-23-3","Texas Instruments","REF3025AIDBZR","SOT-23_3","Top","",1,""]
[null,null,"U8","IC Gate AND 2Ch 4-Inp TSSOP-14","TI","SN74HC21PW","TSSOP-14","Top","",1,""]
[null,null,"U9, U10","42V, 2A Constant On-Time Switching Regulator with Adjustable Current Limit, 10-pin eMSOP, Pb-Free","Texas Instruments","LM25011MYX/NOPB","10-MSOP-EP","Top","",2,""]
[null,null,"U11","Low-Voltage, Precision Comparator, Push-Pull Output","Texas Instruments","LMV761MFX/NOPB","SOT-23_6","Top","",1,""]
[null,null,"U12","Single Power Supply Quadruple Buffer GATE w/ 3-State Output CMOS Logic Level Shifter","Texas Instruments","SN74LV4T125","PW0014A_M","Top","",1,""]
[null,null,"U14","Switched Capacitor Voltage Converter","Texas Instruments","LM2664M6/NOPB","SOT-23_6","Top","",1,""]
[null,null,"U15","Single inverting buffer TSOP5","NXP","74LVC1G04GV,125","TSSOP5","Top","",1,""]
[null,null,"X1, X2","Receptacle 2x20 pins THT 2.54mm pitch","3M","929975-01-20-RK","929975-01-20-RK","Bottom","Yes",2,""]
[null,null,"X3","Micro-Fit 3.0 header 2 pins RA THT","Molex","43650-0200","43650-0200","Bottom","",1,""]
[null,null,"X4","Receptacle 8 pins THT 2.54mm pitch","Molex","22-23-2081","22-23-2081","Bottom","Yes",1,""]
[null,null,"X5, X8, X14","Header 6 pins THT 2.54 mm pitch","Harwin","M20-9990646","HDR-6","Bottom, Bottom, Top","Yes",3,""]
[null,null,"X6","C-GRID III Boxed Header 2p, 2.54mm pitch","Molex","90136-1102","90136-1102","Bottom","Yes",1,""]
[null,null,"X7","C-GRID III Boxed Header 3p, 2.54mm pitch","Molex","90136-1103","90136-1103","Bottom","Yes",1,""]
[null,null,"X9, X11, X13","Test receptacle Red","Harwin","M3498-99","M3498-99","Bottom","Yes",3,""]
[null,null,"X10","Test receptacle Black","Harwin","M3498-98","M3498-98","Bottom","Yes",1,""]
[null,null,"X12","Header 3 pins THT 2.54 mm pitch","Harwin","M20-9990646","HDR-3","Top","Yes",1,""]
[null,null,"X15","Receptacle 2 pins THT 2.54mm pitch","Molex","22-23-2021","22-23-2021","Bottom","Yes",1,""]

{"sheet":"PCB Constraints","index":1,"n_rows":25,"n_cols":7,"rows_kept":25,"flags":["formulas_cached_only"]}
[]
[{"$nulls":3},"PCB production constraints",null,"HSB MRTS"]
[{"$nulls":5},"MLA-0387-A1","PB1"]
[]
[{"$nulls":3},"Project:",null,"MLA-0387-P1.PrjPCB"]
[{"$nulls":3},"Variant:",null,"MLA-0387-A1"]
[null,"Without further notice all components are RoHS compliant"]
[{"$nulls":3},"Report Date:",null,"5-12-2017","16:32:54"]
[{"$nulls":3},"Print Date:",null,"2017-12-05",43074.689753819446]
[null,"Constraint type","Constraint"]
[null,"Dimension","300 x 107.5 mm"]
[null,"Number of layers","4"]
[null,"Minimum clearance","0.15 mm"]
[null,"Minimum track width","0.15 mm"]
[null,"Min finished hole size","0.25 mm"]
[null,"Min annular ring","0.175 mm"]
[null,"Finish","Selective Gold"]
[null,"UR logo","Yes"]
[null,"Color Soldermask","Green"]
[null,"Silkscreen bottom","Yes"]
[null,"Silkscreen color","White"]
[null,"Specific Layer Stackup","No"]
[null,"Edge connectors and surface","No"]
[null,"Board cutouts and minimum drill size","No"]
[null,"Print thickness","1.6 mm"]