{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["BOM"],"not_rendered":{"images":1,"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BOM","index":0,"n_rows":9,"n_cols":7,"rows_kept":9,"merged":[[0,0,2,1],[0,2,2,3],[0,4,0,5],[1,4,1,5],[2,4,2,5]],"flags":["formulas_cached_only"]}
[null,null,"Bill of Materials",null,"Product description",null,"PSU to PCBA Cable Assembly"]
[{"$nulls":4},"Product number",null,"MLA-0387-C2"]
[{"$nulls":4},"Version",null,"PA0"]
["Designator","Description","Manufacturer","Part Number","UL","Quantity","Remark"]
["CB1","Wire 20AWG Black Silicone 5m","Multi-Contact","61.7605-21","",1,"Cut to 55cm"]
["CB2","Wire 20AWG Red Silicone 5m","Multi-Contact","61.7605-22","",1,"Cut to 55cm"]
["M1","Micro-Fit 3.0 Receptacle Housing 2p","Molex","43645-0200","",1,""]
["M2, M4","Crimp Contact Female 20-24AWG Tin","Molex","43030-0001","",2,""]
["M3, M5","Wire Ferrule 0.5mm2","TE Conn","966067-2","",2,""]