{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["BOM"],"not_rendered":{"images":1,"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BOM","index":0,"n_rows":16,"n_cols":7,"rows_kept":16,"merged":[[0,0,2,1],[0,2,2,3],[0,4,0,5],[1,4,1,5],[2,4,2,5]],"flags":["formulas_cached_only"]}
[null,null,"Bill of Materials",null,"Product description",null,"PSU to PCBA Cable Assembly"]
[{"$nulls":4},"Product number",null,"MLA-0387-C2"]
[{"$nulls":4},"Version",null,"PA2"]
["Designator","Description","Manufacturer","Part Number","UL","Quantity","Remark"]
["CB1","Wire 20AWG Black Silicone 30.5m","Alpha Wire","422010 BK005","",1,"Cut to 55cm"]
["CB2","Wire 20AWG Red Silicone 30.5m","Alpha Wire","422010 RD005","",1,"Cut to 55cm"]
["CB3","Wire 20AWG Red Silicone 30.5m","Alpha Wire","422010 RD005","",1,"Cut to 15cm"]
["CB4","Wire 20AWG Black Silicone 30.5m","Alpha Wire","422010 BK005","",1,"Cut to 15cm"]
["CB5","Wire 20AWG Red Silicone 30.5m","Alpha Wire","422010 RD005","",1,"Cut to 12cm"]
["FC1, FC2","Ferrite core, 320R 7.26mm","Laird","28A2025-0A2","",2,""]
["M1","Micro-Fit 3.0 Receptacle Housing 2p","Molex","43645-0200","",1,""]
["M2, M4","Crimp Contact Female 20-24AWG Tin","Molex","43030-0001","",2,""]
["M3, M5","Wire Ferrule 2x20AWG","TE Conn","966144-1","",2,""]
["M6, M9","Female Faston Flag Terminal 18-22 AWG","Molex","0190060001","",2,""]
["M7, M8","Heat shrink tubing, 3.2mm, 2.5:1, black ,1.2m","TE Conn","SCL-1/8-0-STK","",2,"Cut to 10mm length"]
["R1","Resistor, Axial Leaded, 10 ohm, WH Series, 10 W","Welwyn","WH5-10RJI","",1,""]