{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["BOM"],"not_rendered":{"images":1,"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BOM","index":0,"n_rows":15,"n_cols":8,"rows_kept":15,"merged":[[0,0,2,1],[0,2,2,3],[0,6,0,7],[1,6,1,7],[2,6,2,7]],"flags":["formulas_cached_only"]}
[null,null,"Bill of Materials",null,null,"Product description","HSB MRTS Kathode-MCP Front Panel Assembly"]
[{"$nulls":5},"Product number","MLA-0387-M0"]
[{"$nulls":5},"Version","001"]
["Item No.","Description","Manufacturer","Part No.","Revision","Base Part Manufacturer","Base Part No.","Quantity"]
[1,"HSB MRTS Front Panel","MK","MLA-0387-M1","PA0","Elma","21N384",1]
[2,"LCD 20x4 Character display SPI interface","Winstar","WH2004A1-YYH-JW#",{"$nulls":3},1]
[3,"Sealed and Rugged Keypad 16 keys","Storm Interface",70160103,{"$nulls":3},1]
[4,"HSB MRTS Kathode-MCP PCBA","Micro-key","MLA-0387-A0","PA3",null,null,1]
[5,"HEX Spacer 5mm M2","Wurth Elektronik","971 050 244",{"$nulls":3},4]
[6,"HEX Spacer 5mm M2","Wurth Elektronik","971 050 244",{"$nulls":3},6]
[7,"HEX Nut M2 DIN 934","Fabory","01300.020.001",{"$nulls":3},4]
[8,"Hex Nut M3 DIN 934","Fabory","01100.030.001",{"$nulls":3},6]
[9,"M3 Flat Washer DIN 125-1A","Fabory","38100.030.001",{"$nulls":3},6]
[10,"Pan Head Screw Pozidriv M2x4","Fabory","24662.020.004",{"$nulls":3},4]
[11,"DIN 965-Z M3x10","Fabory",24672030010,{"$nulls":3},6]