{"text_format":"3","workbook":"xls","n_sheets":1,"sheets":["BOM"],"not_rendered":{"images":1,"external_links":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"BOM","index":0,"n_rows":14,"n_cols":8,"rows_kept":14,"merged":[[0,0,2,1],[0,2,2,3],[0,6,0,7],[1,6,1,7],[2,6,2,7]],"flags":["formulas_cached_only"]}
[null,null,"Bill of Materials",null,null,"Product description","HSB MRTS Kathode-MCP Front Panel Assembly"]
[{"$nulls":5},"Product number","MLA-0387-M0"]
[{"$nulls":5},"Version","PA1"]
["Item No.","Description","Manufacturer","Part No.","Revision","Base Part Manufacturer","Base Part No.","Quantity"]
[1,"Kathode/MCP Front Panel","Micro-Key","MLA-0387-M11","PA0",null,null,1]
[2,"HSB MRTS Kathode/MCP PCBA","Micro-Key","MLA-0387-A0","PB1",null,null,1]
[3,"Pan Head Screw Pozidriv M2x4","Fabory","24662.020.004",{"$nulls":3},4]
[4,"DIN 965-Z M3x10","Fabory",24672030010,{"$nulls":3},6]
[5,"LCD 20x4 Character display SPI interface","Newhaven","NHD-0420D3Z-FL-GBW-V3",{"$nulls":3},1]
[6,"Sealed and Rugged Keypad 16 keys","Storm Interface",70160103,{"$nulls":3},1]
[7,"Rigid Light Pipe 5mm, Round, low profile 12,7mm length","Bivar","PLW5-500",{"$nulls":3},1]
[8,"PTFE Isolation sheet","Vink","MLA-0387-M7","PA0","Vinplast","PTFE plaat FG-10/2011 XT wit",1]
[9,"Pan Head screw Pozidriv M2,5x8","Fabory",51342025008,{"$nulls":3},4]
[10,"Keypad Cable assembly","Micro-Key","MLA-0387-C0","PA1",null,null,1]